Steps followed after installing the NCPA agent - active check on Nagios Core 3.5.0
[bookmark: _GoBack]1.Check command declaration in Nconf:
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2.Creating New service by setting the check command called check_ncpa and given the following parameters below.
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3.Finally add the service to the host to monitor via NCPA 
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4. On Agent side configuration, I have installed the application NCPA Agent and specify the token that was created from the Nagios server end.

image1.png
Welcome Administrator

Home.

Basic ltems

Modity checkcommand

> Show History

> Show Host parent /child view

> Generate Nagios config

>Hosts Show (Add
> Hostgroups Show /Add
>Services Show {Add
> Advanced Services Show / Add
>Servicegroups  Show / Add
Additional ftems

>08 Show {Add
> Contacts. Show {Add
>Contactgroups  Show / Add
> Checkcommands  Show / Add
>Misccommands  Show / Add
> Timeperiods Show /Add
Advanced ftems

> Host presets Show (Add
>Host templates  Show / Add
> Service templates  Show / Add
>Host deps. Show /Add
>Servicedeps.  Show /Add
Nagios servers

> Central monitors  Show / Add
> Distrib. collectors  Show / Add

check command name
cetauit service name
check commandine
cetauit command params
params descrinon

amount of params

default service.
template(s)

default commandto
depen upon
execution_fallre_erferia
for dependency
natification_falre_erieria
for dependency

USER13/check_nopa -H SHOSTADDRESSS -p 569:

IR

eriable ARG2=Mullple optons - see comma)

2 v

lable ftems

Defaut_colector_server B
Defaut_mantor_server

generc-service

lacal-service

Lotus Netes Services

Netes-service.

sv-pp

/LT YV
WED P

default neme ta use for new services.

separsted by "

Shortdescripton of sach parameter (cormima separsted, same orcer)

selected items
B ackd the folowing
template(s) to all
advancedd.iservices
ket wit tis
checkcommand
(inkedtempites
ere not vishe inthe
GUlbecause they.
ere Inked when the
confiy s generted)

make el servces using the current command dependent an services an
the same host using this command selected here.

the ‘execution_fallre_crieria® value o use forthe dependency; possible
values: o pln]

the natification_falre_ertere value to use for the dependency; passible
values: o pin]




image2.png
Welcome Administrator

Home.

Basic ltems

Modity advanced.service

> Show History

> Show Host parent /child view

> Generate Hagios config

>Hosts Show (Add
> Hostgroups Show /Add
>Services Show {Add
> Advanced Services Show / Add
>Servicegroups  Show / Add
Additional ftems

>08 Show {Add
> Contacts. Show {Add
>Contactgroups  Show / Add
> Checkcommands  Show / Add
>Misccommands  Show / Add
> Timeperiods Show /Add
Advanced ftems

> Host presets Show (Add
>Host templates  Show / Add
> Service templates  Show / Add
>Host deps. Show /Add
>Servicedeps.  Show /Add

Nagios servers

advanced service name
service descrinon
check command

check period

notification perioc

assion advancedtservice
tohast

assion advancedtservice
to hostoroup

CiDrive _ncpa NCont rternal service name

CDrive _nepa

2037 v time periodto run checks

Nagios specific service descripion

2037

time period to larm

available ftems selected items
windows testserver B

EMCSANSwich 2 B

INFSGDCNAGIOS04

MYNADT MY schneider-slectic.com - Decon

WDSGDCETWS2

Accessswich!

Accessswich2

Accessswichd

Accessswichd

/LT YV

available ftems selected items

A Server B
Backup an Storsge.

Cot-a Servers

Cot-A-Servers_NEA

|cat-B.Servers.




image3.png
notes

notes URL
action URL v PNPURL(f nstalec)
max checkatenpts 3 number oftimes toretry checking
check nerval 2 number of [rin ] between reguarly schechled checks.
ety nterval number of [rin ] o wait before scheding a re-check
st ncifcaton clay. Pumber of rin. to wat before sending the frst ncification
natification nerval 50 number of [rin ] o wait before re-nofifying a contact
natification options wuess possible values: wuerfS00]
active checking v doactive checking of services
passive checking v dopassive checking of services
notification enabled 1 v sendnatificatins for services
check freshness. v checkage oflast check resuts
freshness threshold age threshold n [sec.
service parameters
s::ﬁ::ﬂ'ﬂ“’””m ARG1: ISEDDISKSPACE Variable

ARG2: o w078 Muliple optons - see command syrtax




image4.png
widows testerver 2 ciorenem [GRTGAL ] -0z 15050 0 2intin 16s an o




